# hardware config for early beta pixracer boards (prior to R12)

include ../fmuv4/hwdef.dat

# SPI2 SCK is on PB13
#define GPIO_SPI2_SCK	(GPIO_SPI2_SCK_2|GPIO_SPEED_50MHz)
undef SPI2_SCK
undef PB13
PB13 SPI2_SCK SPI2

# note that PC13 (SBUS invert) is active low on this board

# baro is on main sensors bus
undef BARO
SPIDEV ms5611_int2 SPI1 DEVID3  BARO_CS    MODE3  20*MHZ  20*MHZ
BARO MS56XX SPI:ms5611_int2



