# hw definition file for processing by chibios_pins.py
# for Matek F765-Wing bootloader

# MCU class and specific type
MCU STM32F7xx STM32F767xx

# board ID for firmware load
APJ_BOARD_ID 143

# crystal frequency, setup to use external oscillator
OSCILLATOR_HZ 8000000

FLASH_SIZE_KB 2048

# bootloader starts at zero offset
FLASH_RESERVE_START_KB 0

# the location where the bootloader will put the firmware
FLASH_BOOTLOADER_LOAD_KB 96


# order of UARTs (and USB). Allow bootloading on USB and telem1
SERIAL_ORDER OTG1 UART7

# UART7 (telem1)
PE7 UART7_RX UART7
PE8 UART7_TX UART7

# PA10 IO-debug-console
PA11 OTG_FS_DM OTG1
PA12 OTG_FS_DP OTG1

PA13 JTMS-SWDIO SWD
PA14 JTCK-SWCLK SWD

PD10 LED_BOOTLOADER OUTPUT LOW
define HAL_LED_ON 0

define HAL_USE_EMPTY_STORAGE 1
define HAL_STORAGE_SIZE 16384


# Add CS pins to ensure they are high in bootloader
PC4 IMU1_CS CS
PB12 MAX7456_CS CS
PD7 IMU2_CS CS
PE11 SPARE_CS CS
