# hw definition file for processing by chibios_pins.py
# for minimal F405 bootloader

# MCU class and specific type
MCU STM32F4xx STM32F405xx

# board ID for firmware load
APJ_BOARD_ID 125

# crystal frequency
OSCILLATOR_HZ 8000000

FLASH_SIZE_KB 1024

# bootloader is installed at zero offset
FLASH_RESERVE_START_KB 0

# LEDs
PB9 LED_BOOTLOADER OUTPUT LOW
PA14 LED_ACTIVITY  OUTPUT LOW
define HAL_LED_ON 0

# the location where the bootloader will put the firmware
FLASH_BOOTLOADER_LOAD_KB 64


# order of UARTs
SERIAL_ORDER OTG1

PA11 OTG_FS_DM OTG1
PA12 OTG_FS_DP OTG1

define HAL_USE_EMPTY_STORAGE 1
define HAL_STORAGE_SIZE 15360


# Add CS pins to ensure they are high in bootloader
PB10 MAX7456_CS CS
PC1 SDCARD_CS CS
PC0 M25P16_CS CS
PC2 MPU6000_CS CS
