# hw definition file for processing by chibios_hwdef.py
# for F765 bootloader

# MCU class and specific type
MCU STM32F7xx STM32F767xx

# crystal frequency
OSCILLATOR_HZ 16000000

# board ID for firmware load
APJ_BOARD_ID 50

FLASH_SIZE_KB 2048

# bootloader is installed at zero offset
FLASH_RESERVE_START_KB 0

# the location where the bootloader will put the firmware
FLASH_BOOTLOADER_LOAD_KB 32

# enabling PE3 on the Colibri causes it to reset on startup
undef PE3
PE3 VDD_3V3_SENSORS_EN OUTPUT LOW

# SD power is active low on TBS board
undef PG7
undef VDD_3V3_SD_CARD_EN
PG7 nVDD_3V3_SD_CARD_EN OUTPUT HIGH

PC6 LED_BOOTLOADER OUTPUT HIGH
PC7 LED_ACTIVITY OUTPUT HIGH
define HAL_LED_ON 0


# order of UARTs (and USB)
SERIAL_ORDER OTG1 USART2 UART7

# USART2 is telem1
PD6 USART2_RX USART2
PD5 USART2_TX USART2
PD3 USART2_CTS USART2
PD4 USART2_RTS USART2

PF6 UART7_RX UART7 NODMA
PE8 UART7_TX UART7 NODMA

PA11 OTG_FS_DM OTG1
PA12 OTG_FS_DP OTG1

PA13 JTMS-SWDIO SWD
PA14 JTCK-SWCLK SWD

define HAL_USE_EMPTY_STORAGE 1
define HAL_STORAGE_SIZE 16384
