# hw definition file for processing by chibios_pins.py
# for Matek F405-Wing bootloader

# MCU class and specific type
MCU STM32F4xx STM32F405xx

# board ID for firmware load
APJ_BOARD_ID 127

# crystal frequency
OSCILLATOR_HZ 8000000

# bootloader is installed at zero offset
FLASH_RESERVE_START_KB 0

FLASH_SIZE_KB 1024

# the location where the bootloader will put the firmware
FLASH_BOOTLOADER_LOAD_KB 64

define HAL_STORAGE_SIZE 15360
define STORAGE_FLASH_PAGE 1


# order of UARTs
SERIAL_ORDER OTG1 USART1 USART3 UART4 UART5 USART6

PA0 UART4_TX UART4
PA1 UART4_RX UART4

PA9 USART1_TX USART1
PA10 USART1_RX USART1

PA11 OTG_FS_DM OTG1
PA12 OTG_FS_DP OTG1

PC6  USART6_TX USART6
PC7  USART6_RX USART6

PC10 USART3_TX USART3
PC11 USART3_RX USART3

PC12 UART5_TX UART5
PD2  UART5_RX UART5

PA14 LED_BOOTLOADER OUTPUT LOW GPIO(0)
PA13 LED_ACTIVITY OUTPUT LOW GPIO(1) # optional
define HAL_LED_ON 0

# Add CS pins to ensure they are high in bootloader
PA4 MPU_CS CS
PC14 SDCARD_CS CS
PB12 OSD_CS CS
