# FMUv2 build, same as fmuv3, but 1M flash to avoid hardware issue
# with 2nd half of flash on early STM32F427 chips

include ../fmuv3/hwdef.dat

FLASH_SIZE_KB 1024

# this reduces features to keep the firmware small. This is not
# actually needed as of February 2018 as the full build does fit in
# 1M, but it prepares us for when large features such as scripting are
# added to the build
define HAL_MINIMIZE_FEATURES 1

# we don't have a flash page spare to write parameters to:
undef STORAGE_FLASH_PAGE
