# hw definition file for processing by chibios_hwdef.py
# for H743 bootloader

# MCU class and specific type
MCU STM32H7xx STM32H757xx


# USB setup
USB_STRING_MANUFACTURER "ArduPilot"
USB_STRING_PRODUCT "%BOARD%"

define CORE_CM7
define SMPS_PWR

define WATCHDOG_DISABLED

# crystal frequency
OSCILLATOR_HZ 25000000

# board ID for firmware load
APJ_BOARD_ID 146

FLASH_SIZE_KB 2048

# setup build for a peripheral firmware
env AP_PERIPH 1

EXT_FLASH_SIZE_MB 32

# bootloader is installed at zero offset
FLASH_RESERVE_START_KB 0

# the location where the bootloader will put the firmware
# the H743 has 128k sectors
FLASH_BOOTLOADER_LOAD_KB 128

define HAL_LED_ON 1

PK3 LED OUTPUT LOW
PK4 LED_BOOTLOADER OUTPUT
PK5 LED_ACTIVITY OUTPUT

PB15 USART1_RX USART1
PB14 USART1_TX USART1

PA13 JTMS-SWDIO SWD
PA14 JTCK-SWCLK SWD

# the first CAN bus
# PA11 CAN1_RX CAN1
# PA12 CAN1_TX CAN1
# PC8 GPIO CAN_SLEEP OUTPUT LOW

PA11 OTG_FS_DM OTG1
PA12 OTG_FS_DP OTG1


# order of UARTs (and USB)
SERIAL_ORDER OTG1 USART1

# QSPI Flash
PF8 QUADSPI_BK1_IO0 QUADSPI1
PF9 QUADSPI_BK1_IO1 QUADSPI1
PF7 QUADSPI_BK1_IO2 QUADSPI1
PF6 QUADSPI_BK1_IO3 QUADSPI1
PG6 QUADSPI_BK1_NCS QUADSPI1
PB2 QUADSPI_CLK QUADSPI1

# IFace     Device Name     Bus      QSPI Mode     Clk Freq  Size (Pow2)  NCS Delay
QSPIDEV       mt25q       QUADSPI1      MODE1       120*MHZ      24            8

PB13 VBUS INPUT OPENDRAIN


define CAN_APP_NODE_NAME "org.cubepilot.H757"
define BOOTLOADER_DEBUG SD1
