# hw definition file for processing by chibios_pins.py
# for bootloader for mini-pix hardware from RadioLink

# MCU class and specific type
MCU STM32F4xx STM32F405xx

# board ID for firmware load
APJ_BOARD_ID 3

# crystal frequency
OSCILLATOR_HZ 24000000

# flash size
FLASH_SIZE_KB 1024

# don't allow bootloader to use more than 16k
FLASH_USE_MAX_KB 16

# bootloader loads at start of flash
FLASH_RESERVE_START_KB 0

# LEDs
PB1 LED_BOOTLOADER OUTPUT LOW
PE12 LED_ACTIVITY  OUTPUT LOW
define HAL_LED_ON 0

# the location where the bootloader will put the firmware
FLASH_BOOTLOADER_LOAD_KB 16


# order of UARTs (and USB)
SERIAL_ORDER OTG1

# USB pins
PA11 OTG_FS_DM OTG1
PA12 OTG_FS_DP OTG1

# Add CS pins to ensure they are high in bootloader
PC2 LPS22HB_CS CS
PC15 MPU6500_CS CS
PD10 FRAM_CS CS
