###########################################################################################################################################################
# mRo Control Zero F7 Flight Controller
# STM32F777IIK6
# 8x PWM / IO - DMA capable, buffered and level shiftable - 3.3v (default) / 5v Logic
# Front and Rear Connectors: 30pin Molex PicoClasp
# 3x IMUs (BMI088 6DOF, ICM20602 6DOF, ICM20948 9DOF)
# DPS310 Baro, FRAM (256Bb), SDCARD Socket, TC2030 JTAG
# 5x UARTs (2x with hardware flow control), 2x CAN, 1x SPI, 1x I2C
# Onboard 3 color LED and buzzer
# Uncased Weight and Dimensions:
# Weight: 5.3g (.19oz)
# Width:  20mm (.79in)
# Length: 32mm (1.26in)
# M10058 - Initial Release
###########################################################################################################################################################

# MCU class and specific type
MCU STM32F7xx STM32F777xx

# USB setup
USB_STRING_MANUFACTURER "mRo"

# crystal frequency
OSCILLATOR_HZ 24000000

# board ID for firmware load
APJ_BOARD_ID 141

FLASH_SIZE_KB 2048

# bootloader is installed at zero offset
FLASH_RESERVE_START_KB 0

# the location where the bootloader will put the firmware
FLASH_BOOTLOADER_LOAD_KB 96

PB11 LED_BOOTLOADER OUTPUT

# define all 3 to make LED output White.
PB1 LED_ACTIVITY OUTPUT
PB3 LED_ACTIVITY2 OUTPUT
# PB11 LED_ACTIVITY3 OUTPUT

define HAL_LED_ON 0

# order of UARTs (and USB)
SERIAL_ORDER OTG1

PA11 OTG_FS_DM OTG1
PA12 OTG_FS_DP OTG1

PA13 JTMS-SWDIO SWD
PA14 JTCK-SWCLK SWD

# Add CS pins to ensure they are high in bootloader
PC2 ICM_20602_CS CS
PD7 BARO_CS CS
PD10 FRAM_CS CS SPEED_VERYLOW NODMA
PE15 ICM_20948_CS CS
PF10 BMI088_GYRO_CS CS
PF6 BMI088_ACCEL_CS CS
