# hw definition file for processing by chibios_pins.py
# for SP/Racing Extreme H7 hardware.

# MCU class and specific type
MCU STM32H7xx STM32H750xx

# board ID for firmware load
APJ_BOARD_ID 1060

# crystal frequency, setup to use external oscillator
OSCILLATOR_HZ 8000000

# limited flash that can't be used
FLASH_SIZE_KB 128
FLASH_RESERVE_START_KB 0
FLASH_RESERVE_END_KB 0
FLASH_BOOTLOADER_LOAD_KB 128

# 16mb external flash
EXT_FLASH_SIZE_MB 16
EXT_FLASH_RESERVE_START_KB 1024
EXT_FLASH_RESERVE_END_KB 448

# order of UARTs (and USB). Allow bootloading on USB and telem1
SERIAL_ORDER OTG1 USART1

# USART1
PB15 USART1_RX USART1
PB14 USART1_TX USART1

# USB
PA11 OTG_FS_DM OTG1
PA12 OTG_FS_DP OTG1

PA13 JTMS-SWDIO SWD
PA14 JTCK-SWCLK SWD

PE3 LED_BOOTLOADER OUTPUT LOW # Red LED
define HAL_LED_ON 0

# QuadSPI Flash
PD11 QUADSPI_BK1_IO0 QUADSPI1
PD12 QUADSPI_BK1_IO1 QUADSPI1
PE2 QUADSPI_BK1_IO2 QUADSPI1
PD13 QUADSPI_BK1_IO3 QUADSPI1
PB10 QUADSPI_BK1_NCS QUADSPI1
PB2 QUADSPI_CLK QUADSPI1

# IFace  Device Name  Bus      QSPI Mode  Clk Freq  Size (Pow2)  NCS Delay
QSPIDEV  w25q-dtr     QUADSPI1 MODE3      120*MHZ   24           2

define HAL_USE_EMPTY_STORAGE 1
define HAL_STORAGE_SIZE 16384
DEFAULTGPIO OUTPUT LOW PULLDOWN

# Add CS pins to ensure they are high in bootloader
PB12 ICM20602_2_CS CS
PA15 ICM20602_1_CS CS
PE11 AT7456E_CS CS

## pull up VTX power
PB01 VTX_PWR OUTPUT HIGH GPIO(81)
