# setup the four built-in Neopixel LEDs on chan 9
SERVO9_FUNCTION 120
NTF_LED_TYPES 257
NTF_LED_LEN 4

# setup SERIAL3 for RCIN
SERIAL3_PROTOCOL 23

# disable GPS on Serial 4
SERIAL4_PROTOCOL -1

# setup SERIAL6 for GPS
SERIAL6_PROTOCOL 5