# hw definition file for processing by chibios_pins.py
# for DevEBox H7 hardware.

# MCU class and specific type
MCU STM32H7xx STM32H750xx

# board ID for firmware load
APJ_BOARD_ID 1061

# crystal frequency, setup to use external oscillator
OSCILLATOR_HZ 25000000

FLASH_SIZE_KB 128
FLASH_RESERVE_START_KB 0
FLASH_RESERVE_END_KB 0
FLASH_BOOTLOADER_LOAD_KB 128

# 8mb external flash
EXT_FLASH_SIZE_MB 8
EXT_FLASH_RESERVE_START_KB 1024
EXT_FLASH_RESERVE_END_KB 448

# order of UARTs (and USB). Allow bootloading on USB and telem1
SERIAL_ORDER OTG1 USART1 UART7

# UART7 is debug
PE7 UART7_RX UART7 NODMA
PE8 UART7_TX UART7 NODMA
define BOOTLOADER_DEBUG SD7

# QuadSPI Flash
PD11 QUADSPI_BK1_IO0 QUADSPI1
PD12 QUADSPI_BK1_IO1 QUADSPI1
PE2 QUADSPI_BK1_IO2 QUADSPI1
PD13 QUADSPI_BK1_IO3 QUADSPI1
PB6 QUADSPI_BK1_NCS QUADSPI1
PB2 QUADSPI_CLK QUADSPI1

# IFace  Device Name  Bus      QSPI Mode  Clk Freq  Size (Pow2)  NCS Delay
QSPIDEV  w25q         QUADSPI1 MODE3      120*MHZ   23           2

# USART1
PA10 USART1_RX USART1
PA9  USART1_TX USART1

# USB
PA11 OTG_FS_DM OTG1
PA12 OTG_FS_DP OTG1

PA13 JTMS-SWDIO SWD
PA14 JTCK-SWCLK SWD

PA1 LED_BOOTLOADER OUTPUT LOW
define HAL_LED_ON 0

define HAL_USE_EMPTY_STORAGE 1
define HAL_STORAGE_SIZE 16384

# Add CS pins to ensure they are high in bootloader
PA4 MPU6000_CS CS
