# TradHeli Copter3.5 to 3.6 upgrade settings - load with QGC
# Tunes the PSC, LOIT, and Nav for New Loiter and Auto
# Stack: ArduPilot
# Vehicle: Helicopter
# Version: 3.6
# Vehicle-Id Component-Id Name Value Type
1	1	LOIT_ACC_MAX	500	9
1	1	LOIT_ANG_MAX	0	9
1	1	LOIT_BRK_ACCEL	125	9
1	1	LOIT_BRK_DELAY	1	9
1	1	LOIT_BRK_JERK	250	9
1	1	LOIT_SPEED	3000	9
1	1	PHLD_BRAKE_ANGLE	800	4
1	1	PHLD_BRAKE_RATE	4	4
1	1	PSC_ACCZ_D	0	9
1	1	PSC_ACCZ_FF	0	9
1	1	PSC_ACCZ_FILT	20	9
1	1	PSC_ACCZ_FLTD	20	9
1	1	PSC_ACCZ_I	1	9
1	1	PSC_ACCZ_IMAX	800	9
1	1	PSC_ACCZ_P	0.28	9
1	1	PSC_ACC_XY_FILT	2	9
1	1	PSC_ANGLE_MAX	0	9
1	1	PSC_POSXY_P	1	9
1	1	PSC_POSZ_P	1	9
1	1	PSC_VELXY_D	0.0	9
1	1	PSC_VELXY_D_FILT	5	9
1	1	PSC_VELXY_FILT	5	9
1	1	PSC_VELXY_I	0.5	9
1	1	PSC_VELXY_IMAX	1000	9
1	1	PSC_VELXY_P	1	9
1	1	PSC_VELZ_P	5	9
1	1	WPNAV_ACCEL	220	9
1	1	WPNAV_ACCEL_Z	100	9
1	1	WPNAV_SPEED_DN	150	9
1	1	WPNAV_SPEED_UP	250	9
