# hw definition file for processing by chibios_pins.py
# for Mazzy Star Drone bootloader

# MCU class and specific type
MCU STM32F7xx STM32F745xx

# board ID for firmware load
APJ_BOARD_ID 188

# crystal frequency, setup to use external oscillator
OSCILLATOR_HZ 8000000

FLASH_SIZE_KB 1024

# bootloader starts at zero offset
FLASH_RESERVE_START_KB 0

# the location where the bootloader will put the firmware
FLASH_BOOTLOADER_LOAD_KB 96

# board voltage
STM32_VDD 330U

# order of UARTs (and USB)
SERIAL_ORDER OTG1

# PA10 IO-debug-console
PA11 OTG_FS_DM OTG1
PA12 OTG_FS_DP OTG1

PA13 JTMS-SWDIO SWD
PA14 JTCK-SWCLK SWD

PA2 LED_BOOTLOADER OUTPUT LOW
define HAL_LED_ON 0
