# copy this file to .gdbinit in your Firmware tree

# this sets up gdb to use openocd. You must start openocd first
target extended-remote :3333

set mem inaccessible-by-default off
set print pretty

b AP_HAL::panic
b HardFault_Handler
b chSysHalt
set confirm off
