// -*- tab-width: 4; Mode: C++; c-basic-offset: 4; indent-tabs-mode: nil -*-

// use this to prevent recursion during sensor init
static bool in_mavlink_delay;

// this costs us 51 bytes, but means that low priority
// messages don't block the CPU
static mavlink_statustext_t pending_status;

// true when we have received at least 1 MAVLink packet
static bool mavlink_active;

// check if a message will fit in the payload space available
#define CHECK_PAYLOAD_SIZE(id) if (payload_space < MAVLINK_MSG_ID_## id ##_LEN) return false

/*
  !!NOTE!!

  the use of NOINLINE separate functions for each message type avoids
  a compiler bug in gcc that would cause it to use far more stack
  space than is needed. Without the NOINLINE we use the sum of the
  stack needed for each message type. Please be careful to follow the
  pattern below when adding any new messages
 */

static NOINLINE void send_heartbeat(mavlink_channel_t chan)
{
    uint8_t base_mode = MAV_MODE_FLAG_CUSTOM_MODE_ENABLED;
    uint8_t system_status = MAV_STATE_ACTIVE;
    uint32_t custom_mode = control_mode;

    // work out the base_mode. This value is not very useful
    // for APM, but we calculate it as best we can so a generic
    // MAVLink enabled ground station can work out something about
    // what the MAV is up to. The actual bit values are highly
    // ambiguous for most of the APM flight modes. In practice, you
    // only get useful information from the custom_mode, which maps to
    // the APM flight mode and has a well defined meaning in the
    // ArduPlane documentation
    switch (control_mode) {
    case MANUAL:
        base_mode = MAV_MODE_FLAG_MANUAL_INPUT_ENABLED;
        break;
    case LEARNING:
        base_mode = MAV_MODE_FLAG_MANUAL_INPUT_ENABLED;
        break;
    case AUTO:
    case RTL:
    case GUIDED:
    case CIRCLE:
        base_mode = MAV_MODE_FLAG_GUIDED_ENABLED;
        // note that MAV_MODE_FLAG_AUTO_ENABLED does not match what
        // APM does in any mode, as that is defined as "system finds its own goal
        // positions", which APM does not currently do
        break;
    case INITIALISING:
        system_status = MAV_STATE_CALIBRATING;
        break;
    }

#if ENABLE_STICK_MIXING==ENABLED
    if (control_mode != INITIALISING) {
        // all modes except INITIALISING have some form of manual
        // override if stick mixing is enabled
        base_mode |= MAV_MODE_FLAG_MANUAL_INPUT_ENABLED;
    }
#endif

#if HIL_MODE != HIL_MODE_DISABLED
    base_mode |= MAV_MODE_FLAG_HIL_ENABLED;
#endif

    // we are armed if we are not initialising
    if (control_mode != INITIALISING) {
        base_mode |= MAV_MODE_FLAG_SAFETY_ARMED;
    }

    // indicate we have set a custom mode
    base_mode |= MAV_MODE_FLAG_CUSTOM_MODE_ENABLED;

    mavlink_msg_heartbeat_send(
        chan,
        MAV_TYPE_FIXED_WING,
        MAV_AUTOPILOT_ARDUPILOTMEGA,
        base_mode,
        custom_mode,
        system_status);
}

static NOINLINE void send_attitude(mavlink_channel_t chan)
{
    Vector3f omega = ahrs.get_gyro();
    mavlink_msg_attitude_send(
        chan,
        micros(),
        ahrs.roll,
        ahrs.pitch,
        ahrs.yaw,
        omega.x,
        omega.y,
        omega.z);
}

static NOINLINE void send_extended_status1(mavlink_channel_t chan, uint16_t packet_drops)
{
    uint32_t control_sensors_present = 0;
    uint32_t control_sensors_enabled;
    uint32_t control_sensors_health;

    // first what sensors/controllers we have
    control_sensors_present |= (1<<0); // 3D gyro present
    control_sensors_present |= (1<<1); // 3D accelerometer present
    if (g.compass_enabled) {
        control_sensors_present |= (1<<2); // compass present
    }
    control_sensors_present |= (1<<3); // absolute pressure sensor present
    if (g_gps != NULL && g_gps->status() == GPS::GPS_OK) {
        control_sensors_present |= (1<<5); // GPS present
    }
    control_sensors_present |= (1<<10); // 3D angular rate control
    control_sensors_present |= (1<<11); // attitude stabilisation
    control_sensors_present |= (1<<12); // yaw position
    control_sensors_present |= (1<<13); // altitude control
    control_sensors_present |= (1<<14); // X/Y position control
    control_sensors_present |= (1<<15); // motor control

    // now what sensors/controllers are enabled

    // first the sensors
    control_sensors_enabled = control_sensors_present & 0x1FF;

    // now the controllers
    control_sensors_enabled = control_sensors_present & 0x1FF;

    switch (control_mode) {
    case MANUAL:
        break;

    case LEARNING:
        control_sensors_enabled |= (1<<10); // 3D angular rate control
        control_sensors_enabled |= (1<<11); // attitude stabilisation
        break;

    case AUTO:
    case RTL:
        control_sensors_enabled |= (1<<10); // 3D angular rate control
        control_sensors_enabled |= (1<<11); // attitude stabilisation
        control_sensors_enabled |= (1<<12); // yaw position
        control_sensors_enabled |= (1<<13); // altitude control
        control_sensors_enabled |= (1<<14); // X/Y position control
        control_sensors_enabled |= (1<<15); // motor control
        break;

    case INITIALISING:
        break;
    }

    // at the moment all sensors/controllers are assumed healthy
    control_sensors_health = control_sensors_present;

    uint16_t battery_current = -1;
    uint8_t  battery_remaining = -1;

    if (current_total1 != 0 && g.pack_capacity != 0) {
        battery_remaining = (100.0 * (g.pack_capacity - current_total1) / g.pack_capacity);
    }
    if (current_total1 != 0) {
        battery_current = current_amps1 * 100;
    }

    if (g.battery_monitoring == 3) {
        /*setting a out-of-range value.
        It informs to external devices that
        it cannot be calculated properly just by voltage*/
        battery_remaining = 150;
    }

    mavlink_msg_sys_status_send(
        chan,
        control_sensors_present,
        control_sensors_enabled,
        control_sensors_health,
        (uint16_t)(load * 1000),
        battery_voltage1 * 1000, // mV
        battery_current,        // in 10mA units
        battery_remaining,      // in %
        0, // comm drops %,
        0, // comm drops in pkts,
        0, 0, 0, 0);

}

static void NOINLINE send_meminfo(mavlink_channel_t chan)
{
    extern unsigned __brkval;
    mavlink_msg_meminfo_send(chan, __brkval, memcheck_available_memory());
}

static void NOINLINE send_location(mavlink_channel_t chan)
{
    Matrix3f rot = ahrs.get_dcm_matrix(); // neglecting angle of attack for now
    mavlink_msg_global_position_int_send(
        chan,
        millis(),
        current_loc.lat,                // in 1E7 degrees
        current_loc.lng,                // in 1E7 degrees
        g_gps->altitude * 10,             // millimeters above sea level
        (current_loc.alt - home.alt) * 10,           // millimeters above ground
        g_gps->ground_speed * rot.a.x,  // X speed cm/s
        g_gps->ground_speed * rot.b.x,  // Y speed cm/s
        g_gps->ground_speed * rot.c.x,
        g_gps->ground_course);          // course in 1/100 degree
}

static void NOINLINE send_nav_controller_output(mavlink_channel_t chan)
{
    int16_t bearing = nav_bearing / 100;
    mavlink_msg_nav_controller_output_send(
        chan,
        nav_roll / 1.0e2,
        0,
        bearing,
        target_bearing / 100,
        wp_distance,
        altitude_error / 1.0e2,
        groundspeed_error,
        crosstrack_error);
}

static void NOINLINE send_gps_raw(mavlink_channel_t chan)
{
    uint8_t fix = g_gps->status();
    if (fix == GPS::GPS_OK) {
        fix = 3;
    }

    mavlink_msg_gps_raw_int_send(
        chan,
        micros(),
        fix,
        g_gps->latitude,      // in 1E7 degrees
        g_gps->longitude,     // in 1E7 degrees
        g_gps->altitude * 10, // in mm
        g_gps->hdop,
        65535,
        g_gps->ground_speed,  // cm/s
        g_gps->ground_course, // 1/100 degrees,
        g_gps->num_sats);
}

static void NOINLINE send_servo_out(mavlink_channel_t chan)
{
    const uint8_t rssi = 1;
    // normalized values scaled to -10000 to 10000
    // This is used for HIL.  Do not change without discussing with
    // HIL maintainers
 #if X_PLANE == ENABLED
    /* update by JLN for X-Plane or AeroSIM HIL */
    
    int thr_out = constrain((g.channel_throttle.servo_out *2) - 100, -100, 100);  // throttle set from -100 to 100
    mavlink_msg_rc_channels_scaled_send(
        chan,
        millis(),
        0, // port 0
	g.channel_roll.servo_out,
	g.channel_pitch.servo_out,
        100 * thr_out,
	g.channel_rudder.servo_out,
        10000 * g.channel_roll.norm_output(),
        10000 * g.channel_pitch.norm_output(),
        10000 * g.channel_throttle.norm_output(),
        10000 * g.channel_rudder.norm_output(),
        rssi);    
#else
    mavlink_msg_rc_channels_scaled_send(
        chan,
        millis(),
        0, // port 0
        10000 * g.channel_roll.norm_output(),
        10000 * g.channel_pitch.norm_output(),
        10000 * g.channel_throttle.norm_output(),
        10000 * g.channel_rudder.norm_output(),
        0,
        0,
        0,
        0,
        rssi);
#endif
}

static void NOINLINE send_radio_in(mavlink_channel_t chan)
{
    uint8_t rssi = 1;
    mavlink_msg_rc_channels_raw_send(
        chan,
        millis(),
        0, // port
        g.channel_roll.radio_in,
        g.channel_pitch.radio_in,
        g.channel_throttle.radio_in,
        g.channel_rudder.radio_in,
        g.rc_5.radio_in,       // XXX currently only 4 RC channels defined
        g.rc_6.radio_in,
        g.rc_7.radio_in,
        g.rc_8.radio_in,
        rssi);
}

static void NOINLINE send_radio_out(mavlink_channel_t chan)
{
        mavlink_msg_servo_output_raw_send(
            chan,
            micros(),
            0, // port
            APM_RC.OutputCh_current(0),
            APM_RC.OutputCh_current(1),
            APM_RC.OutputCh_current(2),
            APM_RC.OutputCh_current(3),
            APM_RC.OutputCh_current(4),
            APM_RC.OutputCh_current(5),
            APM_RC.OutputCh_current(6),
            APM_RC.OutputCh_current(7));
}

static void NOINLINE send_vfr_hud(mavlink_channel_t chan)
{
    mavlink_msg_vfr_hud_send(
        chan,
        (float)g_gps->ground_speed / 100.0,
        (float)g_gps->ground_speed / 100.0,
        (ahrs.yaw_sensor / 100) % 360,
        (uint16_t)(100 * (g.channel_throttle.norm_output() / 2.0 + 0.5)), // scale -1,1 to 0-100
        current_loc.alt / 100.0,
        0);
}

#if HIL_MODE != HIL_MODE_ATTITUDE
static void NOINLINE send_raw_imu1(mavlink_channel_t chan)
{
    Vector3f accel = ins.get_accel();
    Vector3f gyro = ins.get_gyro();

    mavlink_msg_raw_imu_send(
        chan,
        micros(),
        accel.x * 1000.0 / gravity,
        accel.y * 1000.0 / gravity,
        accel.z * 1000.0 / gravity,
        gyro.x * 1000.0,
        gyro.y * 1000.0,
        gyro.z * 1000.0,
        compass.mag_x,
        compass.mag_y,
        compass.mag_z);
}

static void NOINLINE send_raw_imu3(mavlink_channel_t chan)
{
    Vector3f mag_offsets = compass.get_offsets();
    Vector3f accel_offsets = ins.get_accel_offsets();
    Vector3f gyro_offsets = ins.get_gyro_offsets();

    mavlink_msg_sensor_offsets_send(chan,
                                    mag_offsets.x,
                                    mag_offsets.y,
                                    mag_offsets.z,
                                    compass.get_declination(),
                                    0, 0,
                                    gyro_offsets.x,
                                    gyro_offsets.y,
                                    gyro_offsets.z,
                                    accel_offsets.x,
                                    accel_offsets.y,
                                    accel_offsets.z);
}

static void NOINLINE send_ahrs(mavlink_channel_t chan)
{
    Vector3f omega_I = ahrs.get_gyro_drift();
    mavlink_msg_ahrs_send(
        chan,
        omega_I.x,
        omega_I.y,
        omega_I.z,
        0,
        0,
        ahrs.get_error_rp(),
        ahrs.get_error_yaw());
}

#endif // HIL_MODE != HIL_MODE_ATTITUDE

#ifdef DESKTOP_BUILD
// report simulator state
static void NOINLINE send_simstate(mavlink_channel_t chan)
{
    sitl.simstate_send(chan);
}
#endif

#ifndef DESKTOP_BUILD
static void NOINLINE send_hwstatus(mavlink_channel_t chan)
{
    mavlink_msg_hwstatus_send(
        chan,
        board_voltage(),
        I2c.lockup_count());
}
#endif

static void NOINLINE send_gps_status(mavlink_channel_t chan)
{
    mavlink_msg_gps_status_send(
        chan,
        g_gps->num_sats,
        NULL,
        NULL,
        NULL,
        NULL,
        NULL);
}

static void NOINLINE send_current_waypoint(mavlink_channel_t chan)
{
    mavlink_msg_mission_current_send(
        chan,
        g.command_index);
}

static void NOINLINE send_statustext(mavlink_channel_t chan)
{
    mavlink_msg_statustext_send(
        chan,
        pending_status.severity,
        pending_status.text);
}

// are we still delaying telemetry to try to avoid Xbee bricking?
static bool telemetry_delayed(mavlink_channel_t chan)
{
    uint32_t tnow = millis() >> 10;
    if (tnow > g.telem_delay) {
        return false;
    }
#if USB_MUX_PIN > 0
    if (chan == MAVLINK_COMM_0 && usb_connected) {
        // this is an APM2 with USB telemetry
        return false;
    }
    // we're either on the 2nd UART, or no USB cable is connected
    // we need to delay telemetry
    return true;
#else
    if (chan == MAVLINK_COMM_0) {
        // we're on the USB port
        return false;
    }
    // don't send telemetry yet
    return true;
#endif
}


// try to send a message, return false if it won't fit in the serial tx buffer
static bool mavlink_try_send_message(mavlink_channel_t chan, enum ap_message id, uint16_t packet_drops)
{
    int16_t payload_space = comm_get_txspace(chan) - MAVLINK_NUM_NON_PAYLOAD_BYTES;

    if (telemetry_delayed(chan)) {
        return false;
    }

    switch (id) {
    case MSG_HEARTBEAT:
        CHECK_PAYLOAD_SIZE(HEARTBEAT);
        send_heartbeat(chan);
        return true;

    case MSG_EXTENDED_STATUS1:
        CHECK_PAYLOAD_SIZE(SYS_STATUS);
        send_extended_status1(chan, packet_drops);
        break;

    case MSG_EXTENDED_STATUS2:
        CHECK_PAYLOAD_SIZE(MEMINFO);
        send_meminfo(chan);
        break;

    case MSG_ATTITUDE:
        CHECK_PAYLOAD_SIZE(ATTITUDE);
        send_attitude(chan);
        break;

    case MSG_LOCATION:
        CHECK_PAYLOAD_SIZE(GLOBAL_POSITION_INT);
        send_location(chan);
        break;

    case MSG_NAV_CONTROLLER_OUTPUT:
        if (control_mode != MANUAL) {
            CHECK_PAYLOAD_SIZE(NAV_CONTROLLER_OUTPUT);
            send_nav_controller_output(chan);
        }
        break;

    case MSG_GPS_RAW:
        CHECK_PAYLOAD_SIZE(GPS_RAW_INT);
        send_gps_raw(chan);
        break;

    case MSG_SERVO_OUT:
        CHECK_PAYLOAD_SIZE(RC_CHANNELS_SCALED);
        send_servo_out(chan);
        break;

    case MSG_RADIO_IN:
        CHECK_PAYLOAD_SIZE(RC_CHANNELS_RAW);
        send_radio_in(chan);
        break;

    case MSG_RADIO_OUT:
        CHECK_PAYLOAD_SIZE(SERVO_OUTPUT_RAW);
        send_radio_out(chan);
        break;

    case MSG_VFR_HUD:
        CHECK_PAYLOAD_SIZE(VFR_HUD);
        send_vfr_hud(chan);
        break;

#if HIL_MODE != HIL_MODE_ATTITUDE
    case MSG_RAW_IMU1:
        CHECK_PAYLOAD_SIZE(RAW_IMU);
        send_raw_imu1(chan);
        break;

    case MSG_RAW_IMU3:
        CHECK_PAYLOAD_SIZE(SENSOR_OFFSETS);
        send_raw_imu3(chan);
        break;
#endif // HIL_MODE != HIL_MODE_ATTITUDE

    case MSG_GPS_STATUS:
        CHECK_PAYLOAD_SIZE(GPS_STATUS);
        send_gps_status(chan);
        break;

    case MSG_CURRENT_WAYPOINT:
        CHECK_PAYLOAD_SIZE(MISSION_CURRENT);
        send_current_waypoint(chan);
        break;

    case MSG_NEXT_PARAM:
        CHECK_PAYLOAD_SIZE(PARAM_VALUE);
        if (chan == MAVLINK_COMM_0) {
            gcs0.queued_param_send();
        } else if (gcs3.initialised) {
            gcs3.queued_param_send();
        }
        break;

    case MSG_NEXT_WAYPOINT:
        CHECK_PAYLOAD_SIZE(MISSION_REQUEST);
        if (chan == MAVLINK_COMM_0) {
            gcs0.queued_waypoint_send();
        } else if (gcs3.initialised) {
            gcs3.queued_waypoint_send();
        }
        break;

    case MSG_STATUSTEXT:
        CHECK_PAYLOAD_SIZE(STATUSTEXT);
        send_statustext(chan);
        break;

    case MSG_AHRS:
#if HIL_MODE != HIL_MODE_ATTITUDE
        CHECK_PAYLOAD_SIZE(AHRS);
        send_ahrs(chan);
#endif
        break;

    case MSG_SIMSTATE:
#ifdef DESKTOP_BUILD
        CHECK_PAYLOAD_SIZE(SIMSTATE);
        send_simstate(chan);
#endif
        break;

    case MSG_HWSTATUS:
#ifndef DESKTOP_BUILD
        CHECK_PAYLOAD_SIZE(HWSTATUS);
        send_hwstatus(chan);
#endif
        break;

    case MSG_RETRY_DEFERRED:
        break; // just here to prevent a warning
	}
    return true;
}


#define MAX_DEFERRED_MESSAGES MSG_RETRY_DEFERRED
static struct mavlink_queue {
    enum ap_message deferred_messages[MAX_DEFERRED_MESSAGES];
    uint8_t next_deferred_message;
    uint8_t num_deferred_messages;
} mavlink_queue[2];

// send a message using mavlink
static void mavlink_send_message(mavlink_channel_t chan, enum ap_message id, uint16_t packet_drops)
{
    uint8_t i, nextid;
    struct mavlink_queue *q = &mavlink_queue[(uint8_t)chan];

    // see if we can send the deferred messages, if any
    while (q->num_deferred_messages != 0) {
        if (!mavlink_try_send_message(chan,
                                      q->deferred_messages[q->next_deferred_message],
                                      packet_drops)) {
            break;
        }
        q->next_deferred_message++;
        if (q->next_deferred_message == MAX_DEFERRED_MESSAGES) {
            q->next_deferred_message = 0;
        }
        q->num_deferred_messages--;
    }

    if (id == MSG_RETRY_DEFERRED) {
        return;
    }

    // this message id might already be deferred
    for (i=0, nextid = q->next_deferred_message; i < q->num_deferred_messages; i++) {
        if (q->deferred_messages[nextid] == id) {
            // its already deferred, discard
            return;
        }
        nextid++;
        if (nextid == MAX_DEFERRED_MESSAGES) {
            nextid = 0;
        }
    }

    if (q->num_deferred_messages != 0 ||
        !mavlink_try_send_message(chan, id, packet_drops)) {
        // can't send it now, so defer it
        if (q->num_deferred_messages == MAX_DEFERRED_MESSAGES) {
            // the defer buffer is full, discard
            return;
        }
        nextid = q->next_deferred_message + q->num_deferred_messages;
        if (nextid >= MAX_DEFERRED_MESSAGES) {
            nextid -= MAX_DEFERRED_MESSAGES;
        }
        q->deferred_messages[nextid] = id;
        q->num_deferred_messages++;
    }
}

void mavlink_send_text(mavlink_channel_t chan, gcs_severity severity, const char *str)
{
    if (telemetry_delayed(chan)) {
        return;
    }

    if (severity == SEVERITY_LOW) {
        // send via the deferred queuing system
        pending_status.severity = (uint8_t)severity;
        strncpy((char *)pending_status.text, str, sizeof(pending_status.text));
        mavlink_send_message(chan, MSG_STATUSTEXT, 0);
    } else {
        // send immediately
        mavlink_msg_statustext_send(chan, severity, str);
    }
}

const AP_Param::GroupInfo GCS_MAVLINK::var_info[] PROGMEM = {
    AP_GROUPINFO("RAW_SENS", 0, GCS_MAVLINK, streamRateRawSensors,      0),
	AP_GROUPINFO("EXT_STAT", 1, GCS_MAVLINK, streamRateExtendedStatus,  0),
    AP_GROUPINFO("RC_CHAN",  2, GCS_MAVLINK, streamRateRCChannels,      0),
	AP_GROUPINFO("RAW_CTRL", 3, GCS_MAVLINK, streamRateRawController,   0),
	AP_GROUPINFO("POSITION", 4, GCS_MAVLINK, streamRatePosition,        0),
	AP_GROUPINFO("EXTRA1",   5, GCS_MAVLINK, streamRateExtra1,          0),
	AP_GROUPINFO("EXTRA2",   6, GCS_MAVLINK, streamRateExtra2,          0),
	AP_GROUPINFO("EXTRA3",   7, GCS_MAVLINK, streamRateExtra3,          0),
	AP_GROUPINFO("PARAMS",   8, GCS_MAVLINK, streamRateParams,          0),
    AP_GROUPEND
};


GCS_MAVLINK::GCS_MAVLINK() :
    packet_drops(0),
    waypoint_send_timeout(1000), // 1 second
    waypoint_receive_timeout(1000) // 1 second
{
}

void
GCS_MAVLINK::init(FastSerial * port)
{
    GCS_Class::init(port);
    if (port == &Serial) {
        mavlink_comm_0_port = port;
        chan = MAVLINK_COMM_0;
    }else{
        mavlink_comm_1_port = port;
        chan = MAVLINK_COMM_1;
    }
	_queued_parameter = NULL;
}

void
GCS_MAVLINK::update(void)
{
    // receive new packets
    mavlink_message_t msg;
    mavlink_status_t status;
	status.packet_rx_drop_count = 0;

    // process received bytes
    while (comm_get_available(chan))
    {
        uint8_t c = comm_receive_ch(chan);

#if CLI_ENABLED == ENABLED
        /* allow CLI to be started by hitting enter 3 times, if no
           heartbeat packets have been received */
        if (mavlink_active == 0 && millis() < 20000) {
            if (c == '\n' || c == '\r') {
                crlf_count++;
            } else {
                crlf_count = 0;
            }
            if (crlf_count == 3) {
                run_cli(_port);
            }
        }
#endif

        // Try to get a new message
        if (mavlink_parse_char(chan, c, &msg, &status)) {
            // we exclude radio packets to make it possible to use the
            // CLI over the radio
            if (msg.msgid != MAVLINK_MSG_ID_RADIO) {
                mavlink_active = true;
            }
            handleMessage(&msg);
        }
    }

    // Update packet drops counter
    packet_drops += status.packet_rx_drop_count;

    if (!waypoint_receiving && !waypoint_sending) {
        return;
    }

    uint32_t tnow = millis();

    if (waypoint_receiving &&
        waypoint_request_i <= waypoint_request_last &&
        tnow > waypoint_timelast_request + 500 + (stream_slowdown*20)) {
        waypoint_timelast_request = tnow;
        send_message(MSG_NEXT_WAYPOINT);
    }

    // stop waypoint sending if timeout
    if (waypoint_sending && (millis() - waypoint_timelast_send) > waypoint_send_timeout){
        waypoint_sending = false;
    }

    // stop waypoint receiving if timeout
    if (waypoint_receiving && (millis() - waypoint_timelast_receive) > waypoint_receive_timeout){
        waypoint_receiving = false;
    }
}

// see if we should send a stream now. Called at 50Hz
bool GCS_MAVLINK::stream_trigger(enum streams stream_num)
{
    AP_Int16 *stream_rates = &streamRateRawSensors;
    uint8_t rate = (uint8_t)stream_rates[stream_num].get();

    if (rate == 0) {
        return false;
    }

    if (stream_ticks[stream_num] == 0) {
        // we're triggering now, setup the next trigger point
        if (rate > 50) {
            rate = 50;
        }
        stream_ticks[stream_num] = (50 / rate) + stream_slowdown;
        return true;
    }

    // count down at 50Hz
    stream_ticks[stream_num]--;
    return false;
}

void
GCS_MAVLINK::data_stream_send(void)
{
    if (waypoint_receiving || waypoint_sending) {
        // don't interfere with mission transfer
        return;
    }

    if (_queued_parameter != NULL) {
        if (streamRateParams.get() <= 0) {
            streamRateParams.set(50);
        }
        if (stream_trigger(STREAM_PARAMS)) {
            send_message(MSG_NEXT_PARAM);
        }
        // don't send anything else at the same time as parameters
        return;
    }

    if (stream_trigger(STREAM_RAW_SENSORS)) {
        send_message(MSG_RAW_IMU1);
        send_message(MSG_RAW_IMU3);
    }

    if (stream_trigger(STREAM_EXTENDED_STATUS)) {
        send_message(MSG_EXTENDED_STATUS1);
        send_message(MSG_EXTENDED_STATUS2);
        send_message(MSG_CURRENT_WAYPOINT);
        send_message(MSG_GPS_RAW);            // TODO - remove this message after location message is working
        send_message(MSG_NAV_CONTROLLER_OUTPUT);

        if (last_gps_satellites != g_gps->num_sats) {
            // this message is mostly a huge waste of bandwidth,
            // except it is the only message that gives the number
            // of visible satellites. So only send it when that
            // changes.
            send_message(MSG_GPS_STATUS);
            last_gps_satellites = g_gps->num_sats;
        }
    }

    if (stream_trigger(STREAM_POSITION)) {
        // sent with GPS read
        send_message(MSG_LOCATION);
    }

    if (stream_trigger(STREAM_RAW_CONTROLLER)) {
        send_message(MSG_SERVO_OUT);
    }

    if (stream_trigger(STREAM_RC_CHANNELS)) {
        send_message(MSG_RADIO_OUT);
        send_message(MSG_RADIO_IN);
    }

    if (stream_trigger(STREAM_EXTRA1)) {
        send_message(MSG_ATTITUDE);
        send_message(MSG_SIMSTATE);
    }

    if (stream_trigger(STREAM_EXTRA2)) {
        send_message(MSG_VFR_HUD);
    }

    if (stream_trigger(STREAM_EXTRA3)) {
        send_message(MSG_AHRS);
        send_message(MSG_HWSTATUS);
    }
}



void
GCS_MAVLINK::send_message(enum ap_message id)
{
    mavlink_send_message(chan,id, packet_drops);
}

void
GCS_MAVLINK::send_text(gcs_severity severity, const char *str)
{
    mavlink_send_text(chan,severity,str);
}

void
GCS_MAVLINK::send_text(gcs_severity severity, const prog_char_t *str)
{
    mavlink_statustext_t m;
    uint8_t i;
    for (i=0; i<sizeof(m.text); i++) {
        m.text[i] = pgm_read_byte((const prog_char *)(str++));
    }
    if (i < sizeof(m.text)) m.text[i] = 0;
    mavlink_send_text(chan, severity, (const char *)m.text);
}

void GCS_MAVLINK::handleMessage(mavlink_message_t* msg)
{
    struct Location tell_command = {};                // command for telemetry

    switch (msg->msgid) {

    case MAVLINK_MSG_ID_REQUEST_DATA_STREAM:
        {
            // decode
            mavlink_request_data_stream_t packet;
            mavlink_msg_request_data_stream_decode(msg, &packet);

			if (mavlink_check_target(packet.target_system, packet.target_component))
				break;

            int freq = 0; // packet frequency

			if (packet.start_stop == 0)
				freq = 0; // stop sending
			else if (packet.start_stop == 1)
				freq = packet.req_message_rate; // start sending
			else
				break;

            switch(packet.req_stream_id){

                case MAV_DATA_STREAM_ALL:
                    streamRateRawSensors.set_and_save_ifchanged(freq);
                    streamRateExtendedStatus.set_and_save_ifchanged(freq);
                    streamRateRCChannels.set_and_save_ifchanged(freq);
                    streamRateRawController.set_and_save_ifchanged(freq);
                    streamRatePosition.set_and_save_ifchanged(freq);
                    streamRateExtra1.set_and_save_ifchanged(freq);
                    streamRateExtra2.set_and_save_ifchanged(freq);
                    streamRateExtra3.set_and_save_ifchanged(freq);
                    break;

                case MAV_DATA_STREAM_RAW_SENSORS:
                    streamRateRawSensors = freq;		// We do not set and save this one so that if HIL is shut down incorrectly
														// we will not continue to broadcast raw sensor data at 50Hz.
                    break;
                case MAV_DATA_STREAM_EXTENDED_STATUS:
                    streamRateExtendedStatus.set_and_save_ifchanged(freq);
                    break;

                case MAV_DATA_STREAM_RC_CHANNELS:
                    streamRateRCChannels.set_and_save_ifchanged(freq);
                    break;

                case MAV_DATA_STREAM_RAW_CONTROLLER:
                    streamRateRawController.set_and_save_ifchanged(freq);
                    break;

				//case MAV_DATA_STREAM_RAW_SENSOR_FUSION:
				//    streamRateRawSensorFusion.set_and_save(freq);
				//    break;

                case MAV_DATA_STREAM_POSITION:
                    streamRatePosition.set_and_save_ifchanged(freq);
                    break;

                case MAV_DATA_STREAM_EXTRA1:
                    streamRateExtra1.set_and_save_ifchanged(freq);
                    break;

                case MAV_DATA_STREAM_EXTRA2:
                    streamRateExtra2.set_and_save_ifchanged(freq);
                    break;

                case MAV_DATA_STREAM_EXTRA3:
                    streamRateExtra3.set_and_save_ifchanged(freq);
                    break;

                default:
                    break;
            }
            break;
        }

    case MAVLINK_MSG_ID_COMMAND_LONG:
        {
            // decode
            mavlink_command_long_t packet;
            mavlink_msg_command_long_decode(msg, &packet);
            if (mavlink_check_target(packet.target_system, packet.target_component)) break;

            uint8_t result;

            // do command
            send_text(SEVERITY_LOW,PSTR("command received: "));

            switch(packet.command) {

            case MAV_CMD_NAV_RETURN_TO_LAUNCH:
                set_mode(RTL);
                result = MAV_RESULT_ACCEPTED;
                break;

            case MAV_CMD_MISSION_START:
                set_mode(AUTO);
                result = MAV_RESULT_ACCEPTED;
                break;

            case MAV_CMD_PREFLIGHT_CALIBRATION:
                if (packet.param1 == 1 ||
                    packet.param2 == 1 ||
                    packet.param3 == 1) {
            #if LITE == DISABLED                      
                    startup_INS_ground(true);
            #endif
                }
                if (packet.param4 == 1) {
                    trim_radio();
                }
                result = MAV_RESULT_ACCEPTED;
                break;


            default:
                result = MAV_RESULT_UNSUPPORTED;
                break;
            }

            mavlink_msg_command_ack_send(
                chan,
                packet.command,
                result);

            break;
        }


    case MAVLINK_MSG_ID_SET_MODE:
		{
            // decode
            mavlink_set_mode_t packet;
            mavlink_msg_set_mode_decode(msg, &packet);

            if (!(packet.base_mode & MAV_MODE_FLAG_CUSTOM_MODE_ENABLED)) {
                // we ignore base_mode as there is no sane way to map
                // from that bitmap to a APM flight mode. We rely on
                // custom_mode instead.
                break;
            }
            switch (packet.custom_mode) {
            case MANUAL:
            case LEARNING:
            case AUTO:
            case RTL:
                set_mode(packet.custom_mode);
                break;
            }

            break;
		}

    case MAVLINK_MSG_ID_MISSION_REQUEST_LIST:
        {
            // decode
            mavlink_mission_request_list_t packet;
            mavlink_msg_mission_request_list_decode(msg, &packet);
			if (mavlink_check_target(packet.target_system, packet.target_component))
				break;

            // Start sending waypoints
            mavlink_msg_mission_count_send(
                chan,msg->sysid,
                msg->compid,
                g.command_total + 1); // + home

            waypoint_timelast_send   = millis();
            waypoint_sending         = true;
            waypoint_receiving       = false;
            waypoint_dest_sysid      = msg->sysid;
            waypoint_dest_compid     = msg->compid;
            break;
        }


	// XXX read a WP from EEPROM and send it to the GCS
    case MAVLINK_MSG_ID_MISSION_REQUEST:
        {
            // Check if sending waypiont
            //if (!waypoint_sending) break;
			// 5/10/11 - We are trying out relaxing the requirement that we be in waypoint sending mode to respond to a waypoint request.  DEW

            // decode
            mavlink_mission_request_t packet;
            mavlink_msg_mission_request_decode(msg, &packet);

 			if (mavlink_check_target(packet.target_system, packet.target_component))
 				break;

            // send waypoint
            tell_command = get_cmd_with_index(packet.seq);

            // set frame of waypoint
            uint8_t frame;

			if (tell_command.options & MASK_OPTIONS_RELATIVE_ALT) {
                frame = MAV_FRAME_GLOBAL_RELATIVE_ALT; // reference frame
            } else {
                frame = MAV_FRAME_GLOBAL; // reference frame
            }

            float param1 = 0, param2 = 0 , param3 = 0, param4 = 0;

            uint8_t current = 0; // 1 (true), 0 (false)

			if (packet.seq == (uint16_t)g.command_index)
            	current = 1;

            uint8_t autocontinue = 1; // 1 (true), 0 (false)

            float x = 0, y = 0, z = 0;

            if (tell_command.id < MAV_CMD_NAV_LAST || tell_command.id == MAV_CMD_CONDITION_CHANGE_ALT) {
                // command needs scaling
                x = tell_command.lat/1.0e7; // local (x), global (latitude)
                y = tell_command.lng/1.0e7; // local (y), global (longitude)
                if (tell_command.options & MASK_OPTIONS_RELATIVE_ALT) {
                    z = (tell_command.alt - home.alt) / 1.0e2; // because tell_command.alt already includes a += home.alt
                } else {
                    z = tell_command.alt/1.0e2; // local (z), global/relative (altitude)
                }
            }

			switch (tell_command.id) {				// Switch to map APM command fields inot MAVLink command fields

				case MAV_CMD_NAV_TAKEOFF:
				case MAV_CMD_DO_SET_HOME:
					param1 = tell_command.p1;
					break;

				case MAV_CMD_CONDITION_CHANGE_ALT:
					x=0;	// Clear fields loaded above that we don't want sent for this command
					y=0;
				case MAV_CMD_CONDITION_DELAY:
				case MAV_CMD_CONDITION_DISTANCE:
					param1 = tell_command.lat;
					break;

				case MAV_CMD_DO_JUMP:
					param2 = tell_command.lat;
					param1 = tell_command.p1;
					break;

				case MAV_CMD_DO_REPEAT_SERVO:
					param4 = tell_command.lng;
				case MAV_CMD_DO_REPEAT_RELAY:
				case MAV_CMD_DO_CHANGE_SPEED:
					param3 = tell_command.lat;
					param2 = tell_command.alt;
					param1 = tell_command.p1;
					break;

				case MAV_CMD_DO_SET_PARAMETER:
				case MAV_CMD_DO_SET_RELAY:
				case MAV_CMD_DO_SET_SERVO:
					param2 = tell_command.alt;
					param1 = tell_command.p1;
					break;
			}

			mavlink_msg_mission_item_send(chan,msg->sysid,
										msg->compid,
										packet.seq,
										frame,
										tell_command.id,
										current,
										autocontinue,
										param1,
										param2,
										param3,
										param4,
										x,
										y,
										z);

            // update last waypoint comm stamp
            waypoint_timelast_send = millis();
            break;
        }


    case MAVLINK_MSG_ID_MISSION_ACK:
        {
            // decode
            mavlink_mission_ack_t packet;
            mavlink_msg_mission_ack_decode(msg, &packet);
            if (mavlink_check_target(packet.target_system,packet.target_component)) break;

            // turn off waypoint send
            waypoint_sending = false;
            break;
        }

    case MAVLINK_MSG_ID_PARAM_REQUEST_LIST:
        {
            // decode
            mavlink_param_request_list_t packet;
            mavlink_msg_param_request_list_decode(msg, &packet);
            if (mavlink_check_target(packet.target_system,packet.target_component)) break;

            // Start sending parameters - next call to ::update will kick the first one out

            _queued_parameter = AP_Param::first(&_queued_parameter_token, &_queued_parameter_type);
            _queued_parameter_index = 0;
            _queued_parameter_count = _count_parameters();
            break;
        }

    case MAVLINK_MSG_ID_MISSION_CLEAR_ALL:
        {
            // decode
            mavlink_mission_clear_all_t packet;
            mavlink_msg_mission_clear_all_decode(msg, &packet);
			if (mavlink_check_target(packet.target_system, packet.target_component)) break;

            // clear all commands
            g.command_total.set_and_save(0);

            // note that we don't send multiple acks, as otherwise a
            // GCS that is doing a clear followed by a set may see
            // the additional ACKs as ACKs of the set operations
            mavlink_msg_mission_ack_send(chan, msg->sysid, msg->compid, MAV_MISSION_ACCEPTED);
            break;
        }

    case MAVLINK_MSG_ID_MISSION_SET_CURRENT:
        {
            // decode
            mavlink_mission_set_current_t packet;
            mavlink_msg_mission_set_current_decode(msg, &packet);
            if (mavlink_check_target(packet.target_system,packet.target_component)) break;

            // set current command
            change_command(packet.seq);

            mavlink_msg_mission_current_send(chan, g.command_index);
            break;
        }

    case MAVLINK_MSG_ID_MISSION_COUNT:
        {
            // decode
            mavlink_mission_count_t packet;
            mavlink_msg_mission_count_decode(msg, &packet);
            if (mavlink_check_target(packet.target_system,packet.target_component)) break;

            // start waypoint receiving
            if (packet.count > MAX_WAYPOINTS) {
                packet.count = MAX_WAYPOINTS;
            }
            g.command_total.set_and_save(packet.count - 1);

            waypoint_timelast_receive = millis();
            waypoint_timelast_request = 0;
            waypoint_receiving   = true;
            waypoint_sending     = false;
            waypoint_request_i   = 0;
            waypoint_request_last= g.command_total;
            break;
        }

    case MAVLINK_MSG_ID_MISSION_WRITE_PARTIAL_LIST:
    {
        // decode
        mavlink_mission_write_partial_list_t packet;
        mavlink_msg_mission_write_partial_list_decode(msg, &packet);
        if (mavlink_check_target(packet.target_system,packet.target_component)) break;

        // start waypoint receiving
        if (packet.start_index > g.command_total ||
            packet.end_index > g.command_total ||
            packet.end_index < packet.start_index) {
            send_text(SEVERITY_LOW,PSTR("flight plan update rejected"));
            break;
        }

        waypoint_timelast_receive = millis();
        waypoint_timelast_request = 0;
        waypoint_receiving   = true;
        waypoint_request_i   = packet.start_index;
        waypoint_request_last= packet.end_index;
        break;
    }

#ifdef MAVLINK_MSG_ID_SET_MAG_OFFSETS
    case MAVLINK_MSG_ID_SET_MAG_OFFSETS:
    {
        mavlink_set_mag_offsets_t packet;
        mavlink_msg_set_mag_offsets_decode(msg, &packet);
        if (mavlink_check_target(packet.target_system,packet.target_component)) break;
        compass.set_offsets(Vector3f(packet.mag_ofs_x, packet.mag_ofs_y, packet.mag_ofs_z));
        break;
    }
#endif

	// XXX receive a WP from GCS and store in EEPROM
    case MAVLINK_MSG_ID_MISSION_ITEM:
        {
            // decode
            mavlink_mission_item_t packet;
            uint8_t result = MAV_MISSION_ACCEPTED;

            mavlink_msg_mission_item_decode(msg, &packet);
            if (mavlink_check_target(packet.target_system,packet.target_component)) break;

            // defaults
            tell_command.id = packet.command;

			switch (packet.frame)
			{
				case MAV_FRAME_MISSION:
				case MAV_FRAME_GLOBAL:
					{
						tell_command.lat = 1.0e7*packet.x; // in as DD converted to * t7
						tell_command.lng = 1.0e7*packet.y; // in as DD converted to * t7
						tell_command.alt = packet.z*1.0e2; // in as m converted to cm
						tell_command.options = 0; // absolute altitude
						break;
					}

#ifdef MAV_FRAME_LOCAL_NED
				case MAV_FRAME_LOCAL_NED: // local (relative to home position)
					{
						tell_command.lat = 1.0e7*ToDeg(packet.x/
						(radius_of_earth*cos(ToRad(home.lat/1.0e7)))) + home.lat;
						tell_command.lng = 1.0e7*ToDeg(packet.y/radius_of_earth) + home.lng;
						tell_command.alt = -packet.z*1.0e2;
						tell_command.options = MASK_OPTIONS_RELATIVE_ALT;
						break;
					}
#endif

#ifdef MAV_FRAME_LOCAL
				case MAV_FRAME_LOCAL: // local (relative to home position)
					{
						tell_command.lat = 1.0e7*ToDeg(packet.x/
						(radius_of_earth*cos(ToRad(home.lat/1.0e7)))) + home.lat;
						tell_command.lng = 1.0e7*ToDeg(packet.y/radius_of_earth) + home.lng;
						tell_command.alt = packet.z*1.0e2;
						tell_command.options = MASK_OPTIONS_RELATIVE_ALT;
						break;
					}
#endif

				case MAV_FRAME_GLOBAL_RELATIVE_ALT: // absolute lat/lng, relative altitude
					{
						tell_command.lat = 1.0e7 * packet.x; // in as DD converted to * t7
						tell_command.lng = 1.0e7 * packet.y; // in as DD converted to * t7
						tell_command.alt = packet.z * 1.0e2;
						tell_command.options = MASK_OPTIONS_RELATIVE_ALT; // store altitude relative!! Always!!
						break;
					}

            default:
                result = MAV_MISSION_UNSUPPORTED_FRAME;
                break;
			}

            
            if (result != MAV_MISSION_ACCEPTED) goto mission_failed;

            switch (tell_command.id) {                    // Switch to map APM command fields inot MAVLink command fields
            case MAV_CMD_NAV_WAYPOINT:
            case MAV_CMD_NAV_RETURN_TO_LAUNCH:
                break;

            case MAV_CMD_NAV_TAKEOFF:
            case MAV_CMD_DO_SET_HOME:
                tell_command.p1 = packet.param1;
                break;

            case MAV_CMD_CONDITION_CHANGE_ALT:
                tell_command.lat = packet.param1;
                break;

            case MAV_CMD_CONDITION_DELAY:
            case MAV_CMD_CONDITION_DISTANCE:
                tell_command.lat = packet.param1;
                break;

            case MAV_CMD_DO_JUMP:
                tell_command.lat = packet.param2;
                tell_command.p1 = packet.param1;
                break;

            case MAV_CMD_DO_REPEAT_SERVO:
                tell_command.lng = packet.param4;
            case MAV_CMD_DO_REPEAT_RELAY:
            case MAV_CMD_DO_CHANGE_SPEED:
                tell_command.lat = packet.param3;
                tell_command.alt = packet.param2;
                tell_command.p1 = packet.param1;
                break;

            case MAV_CMD_DO_SET_PARAMETER:
            case MAV_CMD_DO_SET_RELAY:
            case MAV_CMD_DO_SET_SERVO:
                tell_command.alt = packet.param2;
                tell_command.p1 = packet.param1;
                break;

            default:
                result = MAV_MISSION_UNSUPPORTED;
                break;
            }

            if (result != MAV_MISSION_ACCEPTED) goto mission_failed;

			if(packet.current == 2){ 				//current = 2 is a flag to tell us this is a "guided mode" waypoint and not for the mission
				guided_WP = tell_command;

				// add home alt if needed
				if (guided_WP.options & MASK_OPTIONS_RELATIVE_ALT){
					guided_WP.alt += home.alt;
				}

				set_mode(GUIDED);

				// make any new wp uploaded instant (in case we are already in Guided mode)
				set_guided_WP();

				// verify we recevied the command
				mavlink_msg_mission_ack_send(
						chan,
						msg->sysid,
						msg->compid,
						0);

			} else {
				// Check if receiving waypoints (mission upload expected)
				if (!waypoint_receiving) {
                    result = MAV_MISSION_ERROR;
                    goto mission_failed;
                }

				// check if this is the requested waypoint
				if (packet.seq != waypoint_request_i) {
                    result = MAV_MISSION_INVALID_SEQUENCE;
                    goto mission_failed;
                }

                set_cmd_with_index(tell_command, packet.seq);

				// update waypoint receiving state machine
				waypoint_timelast_receive = millis();
                waypoint_timelast_request = 0;
				waypoint_request_i++;

                if (waypoint_request_i > waypoint_request_last) {
					mavlink_msg_mission_ack_send(
						chan,
						msg->sysid,
						msg->compid,
						result);

					send_text(SEVERITY_LOW,PSTR("flight plan received"));
					waypoint_receiving = false;
					// XXX ignores waypoint radius for individual waypoints, can
					// only set WP_RADIUS parameter
				}
			}
            break;

        mission_failed:
            // we are rejecting the mission/waypoint
            mavlink_msg_mission_ack_send(
                chan,
                msg->sysid,
                msg->compid,
                result);
            break;
        }


    case MAVLINK_MSG_ID_PARAM_SET:
        {
            AP_Param                  *vp;
            enum ap_var_type        var_type;

            // decode
            mavlink_param_set_t packet;
            mavlink_msg_param_set_decode(msg, &packet);

			if (mavlink_check_target(packet.target_system, packet.target_component))
				break;

            // set parameter

            char key[AP_MAX_NAME_SIZE+1];
            strncpy(key, (char *)packet.param_id, AP_MAX_NAME_SIZE);
            key[AP_MAX_NAME_SIZE] = 0;

            // find the requested parameter
            vp = AP_Param::find(key, &var_type);
            if ((NULL != vp) &&                             // exists
                    !isnan(packet.param_value) &&               // not nan
                    !isinf(packet.param_value)) {               // not inf

                // add a small amount before casting parameter values
                // from float to integer to avoid truncating to the
                // next lower integer value.
				float rounding_addition = 0.01;

                // handle variables with standard type IDs
                if (var_type == AP_PARAM_FLOAT) {
                    ((AP_Float *)vp)->set_and_save(packet.param_value);
                } else if (var_type == AP_PARAM_INT32) {
                    if (packet.param_value < 0) rounding_addition = -rounding_addition;
                    float v = packet.param_value+rounding_addition;
                    v = constrain(v, -2147483648.0, 2147483647.0);
					((AP_Int32 *)vp)->set_and_save(v);
                } else if (var_type == AP_PARAM_INT16) {
                    if (packet.param_value < 0) rounding_addition = -rounding_addition;
                    float v = packet.param_value+rounding_addition;
                    v = constrain(v, -32768, 32767);
					((AP_Int16 *)vp)->set_and_save(v);
                } else if (var_type == AP_PARAM_INT8) {
                    if (packet.param_value < 0) rounding_addition = -rounding_addition;
                    float v = packet.param_value+rounding_addition;
                    v = constrain(v, -128, 127);
					((AP_Int8 *)vp)->set_and_save(v);
                } else {
                    // we don't support mavlink set on this parameter
                    break;
                }

                // Report back the new value if we accepted the change
                // we send the value we actually set, which could be
                // different from the value sent, in case someone sent
                // a fractional value to an integer type
                mavlink_msg_param_value_send(
                    chan,
                    key,
                    vp->cast_to_float(var_type),
                    mav_var_type(var_type),
                    _count_parameters(),
                    -1); // XXX we don't actually know what its index is...
            }

            break;
        } // end case

    case MAVLINK_MSG_ID_RC_CHANNELS_OVERRIDE:
        {
            // allow override of RC channel values for HIL
            // or for complete GCS control of switch position
            // and RC PWM values.
			if(msg->sysid != g.sysid_my_gcs) break;		// Only accept control from our gcs
            mavlink_rc_channels_override_t packet;
            int16_t v[8];
            mavlink_msg_rc_channels_override_decode(msg, &packet);

			if (mavlink_check_target(packet.target_system,packet.target_component))
				break;

            v[0] = packet.chan1_raw;
            v[1] = packet.chan2_raw;
            v[2] = packet.chan3_raw;
            v[3] = packet.chan4_raw;
            v[4] = packet.chan5_raw;
            v[5] = packet.chan6_raw;
            v[6] = packet.chan7_raw;
            v[7] = packet.chan8_raw;
            rc_override_active = APM_RC.setHIL(v);
			rc_override_fs_timer = millis();
            break;
        }

    case MAVLINK_MSG_ID_HEARTBEAT:
        {
            // We keep track of the last time we received a heartbeat from our GCS for failsafe purposes
			if(msg->sysid != g.sysid_my_gcs) break;
			rc_override_fs_timer = millis();
			pmTest1++;
            break;
        }

	#if HIL_MODE != HIL_MODE_DISABLED
        // This is used both as a sensor and to pass the location
        // in HIL_ATTITUDE mode.
	case MAVLINK_MSG_ID_GPS_RAW_INT:
        {
            // decode
            mavlink_gps_raw_int_t packet;
            mavlink_msg_gps_raw_int_decode(msg, &packet);

            // set gps hil sensor
            g_gps->setHIL(packet.time_usec/1000.0,
                          packet.lat*1.0e-7, packet.lon*1.0e-7, packet.alt*1.0e-3,
                          packet.vel*1.0e-2, packet.cog*1.0e-2, 0, 0);
            break;
        }

        //    Is this resolved? - MAVLink protocol change.....
    case MAVLINK_MSG_ID_VFR_HUD:
        {
            // decode
            mavlink_vfr_hud_t packet;
            mavlink_msg_vfr_hud_decode(msg, &packet);

            // set airspeed
            airspeed = 100*packet.airspeed;
            break;
        }

	case MAVLINK_MSG_ID_HIL_STATE:
		{
			mavlink_hil_state_t packet;
			mavlink_msg_hil_state_decode(msg, &packet);
			
			float vel = sqrt((packet.vx * (float)packet.vx) + (packet.vy * (float)packet.vy));
			float cog = wrap_360(ToDeg(atan2(packet.vx, packet.vy)) * 100);
			
            // set gps hil sensor
            g_gps->setHIL(packet.time_usec/1000.0,
                          packet.lat*1.0e-7, packet.lon*1.0e-7, packet.alt*1.0e-3,
                          vel*1.0e-2, cog*1.0e-2, 0, 0);
			
			#if HIL_MODE == HIL_MODE_SENSORS
			
			// rad/sec
            Vector3f gyros;
            gyros.x = (float)packet.xgyro / 1000.0;
            gyros.y = (float)packet.ygyro / 1000.0;
            gyros.z = (float)packet.zgyro / 1000.0;
            // m/s/s
            Vector3f accels;
            accels.x = (float)packet.xacc / 1000.0;
            accels.y = (float)packet.yacc / 1000.0;
            accels.z = (float)packet.zacc / 1000.0;

            ins.set_gyro(gyros);

            ins.set_accel(accels);
			
			#else

			// set AHRS hil sensor
            ahrs.setHil(packet.roll,packet.pitch,packet.yaw,packet.rollspeed,
            packet.pitchspeed,packet.yawspeed);

			#endif

			break;
		}
#endif
#if HIL_MODE == HIL_MODE_ATTITUDE
    case MAVLINK_MSG_ID_ATTITUDE:
        {
            // decode
            mavlink_attitude_t packet;
            mavlink_msg_attitude_decode(msg, &packet);

            // set AHRS hil sensor
            ahrs.setHil(packet.roll,packet.pitch,packet.yaw,packet.rollspeed,
            packet.pitchspeed,packet.yawspeed);
            break;
        }
#endif
#if HIL_MODE == HIL_MODE_SENSORS

    case MAVLINK_MSG_ID_RAW_IMU:
        {
            // decode
            mavlink_raw_imu_t packet;
            mavlink_msg_raw_imu_decode(msg, &packet);

            // set imu hil sensors
            // TODO: check scaling for temp/absPress
            float temp = 70;
            float absPress = 1;
                  //cliSerial->printf_P(PSTR("accel: %d %d %d\n"), packet.xacc, packet.yacc, packet.zacc);
                  //cliSerial->printf_P(PSTR("gyro: %d %d %d\n"), packet.xgyro, packet.ygyro, packet.zgyro);

            // rad/sec
            Vector3f gyros;
            gyros.x = (float)packet.xgyro / 1000.0;
            gyros.y = (float)packet.ygyro / 1000.0;
            gyros.z = (float)packet.zgyro / 1000.0;
            // m/s/s
            Vector3f accels;
            accels.x = (float)packet.xacc / 1000.0;
            accels.y = (float)packet.yacc / 1000.0;
            accels.z = (float)packet.zacc / 1000.0;

            ins.set_gyro(gyros);

            ins.set_accel(accels);

            compass.setHIL(packet.xmag,packet.ymag,packet.zmag);
            break;
        }

#endif // HIL_MODE

#if MOUNT == ENABLED
    case MAVLINK_MSG_ID_MOUNT_CONFIGURE:
		{
			camera_mount.configure_msg(msg);
			break;
		}

    case MAVLINK_MSG_ID_MOUNT_CONTROL:
		{
			camera_mount.control_msg(msg);
			break;
		}

    case MAVLINK_MSG_ID_MOUNT_STATUS:
		{
			camera_mount.status_msg(msg);
			break;
		}
#endif // MOUNT == ENABLED

    case MAVLINK_MSG_ID_RADIO:
        {
            mavlink_radio_t packet;
            mavlink_msg_radio_decode(msg, &packet);
            // use the state of the transmit buffer in the radio to
            // control the stream rate, giving us adaptive software
            // flow control
            if (packet.txbuf < 20 && stream_slowdown < 100) {
                // we are very low on space - slow down a lot
                stream_slowdown += 3;
            } else if (packet.txbuf < 50 && stream_slowdown < 100) {
                // we are a bit low on space, slow down slightly
                stream_slowdown += 1;
            } else if (packet.txbuf > 95 && stream_slowdown > 10) {
                // the buffer has plenty of space, speed up a lot
                stream_slowdown -= 2;
            } else if (packet.txbuf > 90 && stream_slowdown != 0) {
                // the buffer has enough space, speed up a bit
                stream_slowdown--;
            }
            break;
        }

    } // end switch
} // end handle mavlink

uint16_t
GCS_MAVLINK::_count_parameters()
{
    // if we haven't cached the parameter count yet...
    if (0 == _parameter_count) {
        AP_Param  *vp;
        AP_Param::ParamToken token;

        vp = AP_Param::first(&token, NULL);
        do {
            _parameter_count++;
        } while (NULL != (vp = AP_Param::next_scalar(&token, NULL)));
    }
    return _parameter_count;
}

/**
* @brief Send the next pending parameter, called from deferred message
* handling code
*/
void
GCS_MAVLINK::queued_param_send()
{
    // Check to see if we are sending parameters
    if (NULL == _queued_parameter) return;

    AP_Param      *vp;
    float       value;

    // copy the current parameter and prepare to move to the next
    vp = _queued_parameter;

    // if the parameter can be cast to float, report it here and break out of the loop
    value = vp->cast_to_float(_queued_parameter_type);

    char param_name[AP_MAX_NAME_SIZE];
    vp->copy_name(param_name, sizeof(param_name), true);

    mavlink_msg_param_value_send(
        chan,
        param_name,
        value,
        mav_var_type(_queued_parameter_type),
        _queued_parameter_count,
        _queued_parameter_index);

    _queued_parameter = AP_Param::next_scalar(&_queued_parameter_token, &_queued_parameter_type);
    _queued_parameter_index++;
}

/**
* @brief Send the next pending waypoint, called from deferred message
* handling code
*/
void
GCS_MAVLINK::queued_waypoint_send()
{
    if (waypoint_receiving &&
        waypoint_request_i <= waypoint_request_last) {
        mavlink_msg_mission_request_send(
            chan,
            waypoint_dest_sysid,
            waypoint_dest_compid,
            waypoint_request_i);
    }
}

/*
 a delay() callback that processes MAVLink packets. We set this as the
 callback in long running library initialisation routines to allow
 MAVLink to process packets while waiting for the initialisation to
 complete
*/
static void mavlink_delay(unsigned long t)
{
    uint32_t tstart;
    static uint32_t last_1hz, last_50hz;

    if (in_mavlink_delay) {
        // this should never happen, but let's not tempt fate by
        // letting the stack grow too much
        delay(t);
        return;
    }

    in_mavlink_delay = true;

    tstart = millis();
    do {
        uint32_t tnow = millis();
        if (tnow - last_1hz > 1000) {
            last_1hz = tnow;
            gcs_send_message(MSG_HEARTBEAT);
            gcs_send_message(MSG_EXTENDED_STATUS1);
        }
        if (tnow - last_50hz > 20) {
            last_50hz = tnow;
            gcs_update();
        }
        delay(1);
#if USB_MUX_PIN > 0
        check_usb_mux();
#endif
    } while (millis() - tstart < t);

    in_mavlink_delay = false;
}

/*
  send a message on both GCS links
 */
static void gcs_send_message(enum ap_message id)
{
    gcs0.send_message(id);
    if (gcs3.initialised) {
        gcs3.send_message(id);
    }
}

/*
  send data streams in the given rate range on both links
 */
static void gcs_data_stream_send(void)
{
    gcs0.data_stream_send();
    if (gcs3.initialised) {
        gcs3.data_stream_send();
    }
}

/*
  look for incoming commands on the GCS links
 */
static void gcs_update(void)
{
	gcs0.update();
    if (gcs3.initialised) {
        gcs3.update();
    }
}

static void gcs_send_text_P(gcs_severity severity, const prog_char_t *str)
{
    gcs0.send_text(severity, str);
    if (gcs3.initialised) {
        gcs3.send_text(severity, str);
    }
}

/*
  send a low priority formatted message to the GCS
  only one fits in the queue, so if you send more than one before the
  last one gets into the serial buffer then the old one will be lost
 */
static void gcs_send_text_fmt(const prog_char_t *fmt, ...)
{
    char fmtstr[40];
    va_list ap;
    uint8_t i;
    for (i=0; i<sizeof(fmtstr)-1; i++) {
        fmtstr[i] = pgm_read_byte((const prog_char *)(fmt++));
        if (fmtstr[i] == 0) break;
    }
    fmtstr[i] = 0;
    pending_status.severity = (uint8_t)SEVERITY_LOW;
    va_start(ap, fmt);
    vsnprintf((char *)pending_status.text, sizeof(pending_status.text), fmtstr, ap);
    va_end(ap);
    mavlink_send_message(MAVLINK_COMM_0, MSG_STATUSTEXT, 0);
    if (gcs3.initialised) {
        mavlink_send_message(MAVLINK_COMM_1, MSG_STATUSTEXT, 0);
    }
}

