#NOTE: 2014-11-13 Frame : 3DR_X8-M_RTF ArduCopter_3.2
ACRO_BAL_PITCH,1
ACRO_BAL_ROLL,1
ACRO_EXPO,0.3
ACRO_RP_P,4.5
ACRO_TRAINER,2
ACRO_YAW_P,3
ANGLE_MAX,4500
ATC_ACCEL_RP_MAX,72000
ATC_ACCEL_Y_MAX,18000
ATC_RATE_FF_ENAB,1
ATC_RATE_RP_MAX,9000
ATC_RATE_Y_MAX,9000
ATC_SLEW_YAW,1000
BATT_AMP_PERVOLT,17
BATT_CAPACITY,10000
BATT_CURR_PIN,3
BATT_MONITOR,4
BATT_VOLT_MULT,10.1
BATT_VOLT_PIN,2
CAM_DURATION,1
CAM_TRIGG_DIST,0
CAM_TRIGG_TYPE,1
CH7_OPT,18
CH8_OPT,0
COMPASS_ORIENT,0
FENCE_ACTION,1
FENCE_ALT_MAX,100
FENCE_ENABLE,1
FENCE_MARGIN,2
FENCE_RADIUS,300
FENCE_TYPE,3
FLTMODE1,0
FLTMODE2,5
FLTMODE3,3
FLTMODE4,0
FLTMODE5,2
FLTMODE6,6
FRAME,1
FS_BATT_ENABLE,1
FS_BATT_VOLTAGE,14
FS_GPS_ENABLE,1
FS_THR_ENABLE,1
GPS_HDOP_GOOD,200
HLD_LAT_P,1
LAND_REPOSITION,1
LOG_BITMASK,-6146
LOITER_LAT_D,0
LOITER_LAT_I,0.5
LOITER_LAT_IMAX,1000
LOITER_LAT_P,1
LOITER_LON_D,0
LOITER_LON_I,0.5
LOITER_LON_IMAX,1000
LOITER_LON_P,1
MNT_ANGMAX_TIL,0
MNT_ANGMIN_TIL,-9000
MNT_MODE,3
MNT_RC_IN_TILT,6
MOT_SPIN_ARMED,70
PILOT_ACCEL_Z,250
PILOT_VELZ_MAX,250
RATE_PIT_D,0.02
RATE_PIT_I,0.3
RATE_PIT_IMAX,1000
RATE_PIT_P,0.3
RATE_RLL_D,0.02
RATE_RLL_I,0.35
RATE_RLL_IMAX,1000
RATE_RLL_P,0.35
RATE_YAW_D,0.005
RATE_YAW_I,0.02
RATE_YAW_IMAX,1000
RATE_YAW_P,0.16
RC_FEEL_RP,15
RC9_FUNCTION,7
RC9_MAX,1520
RC9_MIN,1000
RC9_REV,1
RELAY_PIN,55
RTL_ALT,2000
SERIAL2_PROTOCOL,2
STB_PIT_P,6.6484
STB_RLL_P,7.6484
STB_YAW_P,2.5
THR_ACCEL_D,0
THR_ACCEL_I,1
THR_ACCEL_IMAX,800
THR_ACCEL_P,0.5
THR_ALT_P,1
THR_DZ,100
THR_MAX,1000
THR_MID,450
THR_MIN,130
THR_RATE_P,5
WPNAV_ACCEL,250
WPNAV_ACCEL_Z,100
WPNAV_LOIT_JERK,1000
WPNAV_LOIT_SPEED,1000
WPNAV_RADIUS,200
WPNAV_SPEED,650
WPNAV_SPEED_DN,150
WPNAV_SPEED_UP,250
